**TITLE**: Instruction for Inspection and Testing of PA79/696 PCB for 400A model

(DUAL DISPLAY) (WITH SHUNT).

(ERP CODE: **D17.01.008.0386**)

**1 SCOPE:**

Applicable for testing of 400A model with SHUNT

(ERP CODE: D17.01.008.0386 DUAL DISPLAY)

**2 DETAILS OF THE INSTRUCTION:**

2.1 Inspection / Measuring / Test Equipment:

2.1.1 Digital Multimeter.

2.1.2 Wire boom for test.

2.1.4 Record the test results (OK / NOT OK) in the test report as the testing progress. (REF: INSP ).

**3** **VISUAL INSPECTION:**

3.1 Check the components on the PCB according to BOM.

**4 ELECTRICAL TEST:**

**Note: After testing keep toggle switches and knobs to their default position.**

**4.1 NO LOAD TEST:**

4.1.1 Switch ON power supply of TEST JIG***.*** Keep +VE/ -VE current Feedback toggle switch at -VE

4.1.2 Keep SHUNT/HALL SENSOR switch to SHUNT position and keep VOLT/ISOLATOR toggle switch on TEST JIG in VOLT position.

4.1.3 Vary FEEDBACK CURRENT POT from MIN to MAX position and check voltage at respective test point (from 0mV-75mV) on TEST JIG.

4.1.4 Vary FEEDBACK VOLTAGE POT from MIN to MAX position and check voltage at respective test point (from 0V-20V (+/- 2V)) on TEST JIG.

4.1.5 Now switch off the TEST JIG and connect ADON PCB test jig to regular Champ Multi display PCB test jig. Connect all connectors to test PCB. Switch ON the power supply.

4.1.6 LD1 (Green LED) will be ON when display PCB is switched ON the regular display Pcb test jig.

4.1.7 Now check the voltage levels at the test points with respect to ground as follows on Test PCB.

|  |  |
| --- | --- |
| **TEST POINT** | **VOLTAGE** |
| TP1 | +5 Volt |
| TP2 | GND |

* + 1. Program the TEST PCB

***(Microcontroller – PIC18F46K40 and Programming connector CN6 on TEST PCB. Match Pin 1 of both Pickit and CN6)***

**Note: Ensure the correct software revision is displayed during power on of PCB.**

* + 1. Switch off the supply. Remove connector CN7 of test PCB & then switch ON the power supply.
    2. For D17.01.008.0386 PCB it shows SET CURRENT/ FEEDBACK CURRENT and ACTUAL VOLATGE (FEEDBACK VOLTAGE).
    3. Set CURRENT POT (P1), ARC FORCE POT (P2), HOTSTART POT (P3) at MIN position.
    4. Set the 1VDC at P4 (+VE) & P5 (+VE) (banana socket) wrt GND (banana socket) with help of P4 & P5 pot respectively.

**4.2** **KEY FUNCTIONALITY:**

4.2.1 Toggle MMA/TIG switch to change mode from MMA to TIG or vice versa. Display indicates the change by showing respective mode on display.

**4.3 CURRENT CALIBRATION in MMA mode:**

4.3.1 Keep MMA/ TIG mode switch at MMA position. Keep the VOLTAGE FEEDBACK pot on MAX (20VDC+/-2VDC).

4.3.2 Check set current on display by varying CURRENT POT (P1)

(Note: Increase or decrease the set current by varying CURRENT POT (P1) in clockwise or anticlockwise direction. The intensity of REF led on main test jig must go on increasing with increasing set current and vice versa. If the REF led does not work, check voltage at TP8 (0 to 2.3V ±1V) w.r.t TP2.)

|  |  |
| --- | --- |
| **MODEL** | **400A** |
| **MIN CURRENT** | 10A |
| **MAX CURRENT** | 400A |

4.3.3 Keep CURRENT POT (P1) at max position. Now rotate the FEEDBACK CURRENT pot at maximum position (75mV) on main TEST JIG, current on display should be set according to the model selected. To calibrate the feedback current on display, use pot ‘VR1’of display PCB to set 400A on display. (Anticlockwise decrease, Clockwise increase)

4.3.4 Keep CURRENT POT (P1), FEEDBACK CURRENT pot at Min position.

**4.4 VOLTAGE CALIBRATION in MMA mode:**

4.4.1 Keep MMA/ TIG mode switch MMA position.

4.4.2 **(only for 017.01.008.0347) (Anticlockwise decrease, Clockwise increase).** Voltage on seven segment display should show voltage same as that at FEEDBACK VOLTAGE terminals on test jig. If not, adjust using VR2 pot

##### 4.5 CURRENT CALIBRATION IN MMA/TIG MODE WITH REMOTE:

4.5.1 Keep MMA/ TIG mode switch at MMA position. Connect CN7 connector to the test PCB. With the help of REMOTE POT current can be varied within the following limits.

|  |  |
| --- | --- |
| **MODEL** | **400A** |
| **MIN CURRENT** | 10A |
| **MAX CURRENT** | 400A |

4.5.2 Keep MMA/ TIG mode switch at TIG position. With the help of REMOTE POT current can be varied same as above table.

4.5.3 Remove the CN7 connector & keep MMA/ TIG mode switch at MMA position.

**4.6 HOT START mode: (TP5=2.3V)**

4.6.1 Keep CURRENT FEEDBACK POT at MIN position & VOLTAGE FEEDBACK at MAX position on TEST JIG. Keep MMA/TIG switch at MMA mode.

4.6.2 SET CURRENT to 100A by CURRENT POT (P1) and HOT START POT(P3) to MAX position.

For 017.01.008.0352, set TP5 at 2.3VDC (+/-0.2VDC) using VR2 pot.

For 017.01.008.0347, set FEEDBACK VOLTAGE on seven segments above 31V using VR2 pot**.**

4.6.3 Rotate the CURRENT FEDBACK pot towards MAX. Voltage at TP8 will be Decreased for 1.5s from the time FEEDBACK CURRENT is given. This means HOT START mode is on.

4.6.3 Rotate the HOT START pot, CURRENT FEEDBACK POT towards MIN position. & Keep other setting as it is.

**4.7 VRD mode in MMA mode:**

4.7.1 Set FEEDBACK VOLTAGE POT at maximum position by keeping TP5 = 2.3V (+/- 0.5VDC) using VR2 POT (for 017.01.008.0352)

Set FEEDBACK VOLTAGE above 70V on voltage seven segment using VR2 POT (for 017.01.008.0347)

4.7.2 Press rocker switch VRD ON/VRD OFF to select VRD ON. Wait for 2 sec, then Monitor LD2 or SHDN led on test jig. The LED should glow. Default time is 2 sec

4.7.3 Press VRD switch to select VRD OFF. LD2 & SHDN led will remain off.

4.7.4 Check 3 minute VRD time for 10% of the PCBs in the batch by changing the VRD time as below. Please mention the PCB sr. no in the report.

* If timing to be changed, turn OFF the power supply of jig & then short JP1 & now put the VRD switch in ON condition & then turn ON the power supply of jig.
* In place of set current display show VRD count.
* Default count will be 000 as 2sec.Set the count to 18 with help of HOT START (P3) pot.
* Remove JP1 and set current will be displayed again. Check the VRD function now**. (VRD LED will be glow ON after three minutes.)**
* After testing, set VRD time to 2 sec default time. Using jumper JP1 and set the time 000 on seven segment display of test PCB using HOTSTART pot P3.

4.7.5 **VRD Mode is only applicable in MMA mode**. In TIG mode VRD mode is disabled. LD2 will not glow in TIG MODE.

**4.8 ARC FORCE mode:**

4.8.1 Keep CURRENT FEEDBACK POT on main JIG at minimum position (TP5=0.6V). Rotate the ARC FORCE pot at max position. Now rotate FEEDBACK VOLTAGE pot of TEST JIG towards MIN.

4.8.2 Voltage at TP8 will be gradually increased as FEEDBACK VOLTAGE on seven segment is decreasing from 30V to 10V (For 017.01.008.0347).

4.8.3 Voltage at TP8 will be gradually increased as VOLTAGE FEEDBACK on test jig (banana socket) is decreasing up to 10V. (For 017.01.008.0352).

4.8.4 This means ARCFORCE mode is on.

4.8.5 Now decrease FEEDBACK VOLTAGE pot of TEST JIG below 10V, voltage at TP8 will be remain constant. This means ANTISTICK mode is on.

4.8.6 Keep the ARC FORCE POT at MIN position. VOLTAGE FEEDBACK at MAX position

**4.9 TIG mode**

4.9.1Press MMA/TIG switch to select TIG mode.

4.9.2 Check set current on display by varying CURRENT POT (P1). (Note: Increase or decrease the set current by rotating pot P1 in clockwise or anticlockwise direction, intensity of REF led must go on increasing with increasing set current and vice versa. If the REF led does not work, check voltage at TP8 w.r.t TP2).

4.9.3 Rotate the FEEDBACK CURRENT pot on TEST JIG, current on display should vary from 10A-400A, indicating welding is ON.

**4.10 TRIP SECTION**

4.10.1 By rotating P4 & P5 observe the following error message on display.

4.10.2 After Checking Sr. no 1 & 2, set P4(+ve) at 1VDC & check next points.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Sr. No** | **Error code** | **Use pot** | **Voltage (VDC) wrt GND (banana Socket)** | | **Error description** |
| 1 | Err 001 | P4 | **Across P4 (+ve)**  **(+/-0.05)** | 2.9– 3.9 | Under Voltage |
| 2 | Err 003 | P4 | 4.3– 4.65 | Thermal Error |
| 3 | Err 002 | P5 | **Across P5 (+ve)**  **(+/-0.05)** | 3.7– 5 | Over Voltage |

**4.11 PCB tested successfully.**

**Prepared By, Approved By,**

**Jeetendra Kadam Mr. Sachin Dobhada**

(16/02/2023)